{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Capacité de transport"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Capacité de transport","index":0,"n_rows":7,"n_cols":9,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,"Diamètre nominal             \nDN (mm)","Longueur                  \nL (m)","Rugosité fonctionnelle\nkb (mm)","Débit                       \nQ (l/s)","Pertes de charge                 \nΔH (mCE)",null,"Somme de contrôle"]
[null,null,100,800,0.1,{"$f":"40/3.6","v":11.111111111111111},17.953862425499338,null,{"$f":"IF(OR(C4=0,G4=0),-F4,IF(D4=0,9.99999999999999E+99,PI()*POWER(C4/1000,2)/4*(-2*LOG(0.000003263/SQRT(19.6133*POWER(C4/1000,3)*G4/D4)+E4/(3.71*C4/1000*1000),10)*SQRT(19.6133*C4/1000*G4/D4))*1000-F4))","v":-2.6464341829068871E-9}]
[]
[null,null,"Rendement pompe             \nη (%)","Hauteur géodésique                  \nHgeo (m)","Puissance                  \nP (kW)","Energie spécifique                  \nE (kWh/m3)"]
[null,null,70,180,{"$f":"(D7+G4)*(F4/1000)*9.80655/(C7/100)","v":30.813403961409211},{"$f":"E7/(F4*3.6)","v":0.77033509903523023}]